# antenna_diversity Struct Reference
[MM]

Antenna Diversity structure. More...

`#include <mm.h>`

## Data Fields
bool | enable
| Boolean indicating if the algorithm is enabled.
bool | sw_enable
| Boolean indicating if the antenna can be switched.
int8_t | rssi [2]
| Current RSSI.
int8_t | init_rssi [2]
| Initial RSSI.
uint8_t | cur_ant
| Current antenna.
bool | init_rssi_upd_req
| Boolean indicating if the RSSI should be updated.
uint32_t | update_cnt
| Counter of beacon periods spent without any antenna switch outside of the golden range.
uint8_t | nvif_active
| Counter of active VIFs.

## Detailed Description

Antenna Diversity structure.

Definition at line 290 of file mm.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/mm/mm.h