# sm_env_tag Struct Reference
[SM]

station environment structure More...

`#include <sm.h>`

Collaboration diagram for sm_env_tag:
[legend]

## Data Fields
struct sm_connect_req const * | connect_param
| Pointer to the connection parameters.
struct sm_connect_ind * | connect_ind
| Pointer to the structure used for the connect indication upload.
struct ke_msg * | disconnect_ind
| Pointer to the message structure used for the disconnect indication.
struct co_list | bss_config
| List of BSS configuration messages to send.
bool | host_disconnect
| Indicate if pending disconnection was requested by host or not.
bool | join_passive
| Indicate if passive scan has been used during join procedure.
bool | ft_over_ds
| FT over DS is ongoing.
struct mac_addr | ft_old_bssid
| MAC address of old AP - during FT over DS transition.
struct vif_info_tag * | vif_disconnect
| Pointer to the VIF structure for which the disconnection procedure is pending.

## Detailed Description

station environment structure

Definition at line 35 of file sm.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/sm/sm.h