# txl_buffer_control Struct Reference
[TX_SWDESC]

Control descriptor containing information about the transmission rates to use, the Beamforming/HTC/STBC flags, etc. More...

`#include <tx_swdesc.h>`

Collaboration diagram for txl_buffer_control:
[legend]

## Data Fields
union {
struct tx_policy_tbl policy_tbl
| Policy table (filled by the upper MAC).
struct tx_compressed_policy_tbl comp_pol_tbl
| Compressed policy table (used for MU-MIMO if enabled).
}; |
uint32_t | mac_control_info
| MAC Control Information field (filled by the upper MAC).
uint32_t | phy_control_info
| PHY Control Information field (filled by the upper MAC).
uint32_t | tx_flags
| Flags from UMAC which do not fit with tx_hd.macctrlinfo2 format (see tx_swdesc_umac_flags).

## Detailed Description

Control descriptor containing information about the transmission rates to use, the Beamforming/HTC/STBC flags, etc.

Definition at line 82 of file tx_swdesc.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/tx/tx_swdesc.h