# mm_tim_update_req Struct Reference
[MM_TASK]

Structure containing the parameters of the MM_TIM_UPDATE_REQ message. More...

`#include <mm_task.h>`

## Data Fields
uint16_t | aid
| Association ID of the STA the bit of which has to be updated (0 for BC/MC traffic).
uint8_t | tx_avail
| Flag indicating the availability of data packets for the given STA.
uint8_t | inst_nbr
| Index of the VIF for which the TIM is updated.

## Detailed Description

Structure containing the parameters of the MM_TIM_UPDATE_REQ message.

Definition at line 789 of file mm_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/mm/mm_task.h