# mm_channel_switch_ind Struct Reference
[MM_TASK]

Structure containing the parameters of the MM_CHANNEL_SWITCH_IND message. More...

`#include <mm_task.h>`

## Data Fields
uint8_t | chan_index
| Index of the channel context we will switch to.
bool | roc
| Indicate if the switch has been triggered by a Remain on channel request.
uint8_t | vif_index
| VIF on which remain on channel operation has been started (if roc == 1).
bool | roc_tdls
| Indicate if the switch has been triggered by a TDLS Remain on channel request.

## Detailed Description

Structure containing the parameters of the MM_CHANNEL_SWITCH_IND message.

Definition at line 663 of file mm_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/mm/mm_task.h