------------------------------------------------------------------------------------
--------------------- Entries for 1x1 20 MHz 11n/ac/ax no STBC ---------------------
------------------------------------------------------------------------------------
Index   0, RAM Address    0 -    4 : 11n/ac datarate    8.0 Mbps @ rate 0, mStbc = 0
Index   1, RAM Address    5 -    9 : 11n/ac datarate   15.0 Mbps @ rate 0, mStbc = 0
Index   2, RAM Address   10 -   14 : 11n/ac datarate   29.0 Mbps @ rate 0, mStbc = 0
Index   3, RAM Address   15 -   19 : 11n/ac datarate   58.0 Mbps @ rate 1, mStbc = 0
Index   4, RAM Address   20 -   24 : 11n/ac datarate   22.0 Mbps @ rate 2, mStbc = 0
Index   5, RAM Address   25 -   29 : 11n/ac datarate   44.0 Mbps @ rate 2, mStbc = 0
Index   6, RAM Address   30 -   34 : 11n/ac datarate   65.0 Mbps @ rate 2, mStbc = 0
Index   7, RAM Address   35 -   39 : 11n/ac datarate   87.0 Mbps @ rate 2, mStbc = 0
Index   8, RAM Address   40 -   44 : 11n/ac datarate   73.0 Mbps @ rate 3, mStbc = 0
Index   9, RAM Address   45 -   49 :   11ax datarate    0.4 Mbps @ rate 0, mStbc = 0
Index  10, RAM Address   50 -   54 :   11ax datarate    0.9 Mbps @ rate 0, mStbc = 0
Index  11, RAM Address   55 -   59 :   11ax datarate    1.8 Mbps @ rate 0, mStbc = 0
Index  12, RAM Address   60 -   64 :   11ax datarate    1.9 Mbps @ rate 0, mStbc = 0
Index  13, RAM Address   65 -   69 :   11ax datarate    3.5 Mbps @ rate 0, mStbc = 0
Index  14, RAM Address   70 -   74 :   11ax datarate    3.7 Mbps @ rate 0, mStbc = 0
Index  15, RAM Address   75 -   79 :   11ax datarate    4.3 Mbps @ rate 0, mStbc = 0
Index  16, RAM Address   80 -   84 :   11ax datarate    7.1 Mbps @ rate 0, mStbc = 0
Index  17, RAM Address   85 -   89 :   11ax datarate    7.5 Mbps @ rate 0, mStbc = 0
Index  18, RAM Address   90 -   94 :   11ax datarate    8.6 Mbps @ rate 0, mStbc = 0
Index  19, RAM Address   95 -   99 :   11ax datarate   15.0 Mbps @ rate 0, mStbc = 0
Index  20, RAM Address  100 -  104 :   11ax datarate   17.2 Mbps @ rate 0, mStbc = 0
Index  21, RAM Address  105 -  109 :   11ax datarate   34.4 Mbps @ rate 0, mStbc = 0
Index  22, RAM Address  110 -  114 :   11ax datarate    7.1 Mbps @ rate 1, mStbc = 0
Index  23, RAM Address  115 -  119 :   11ax datarate   14.1 Mbps @ rate 1, mStbc = 0
Index  24, RAM Address  120 -  124 :   11ax datarate   30.0 Mbps @ rate 1, mStbc = 0
Index  25, RAM Address  125 -  129 :   11ax datarate   68.8 Mbps @ rate 1, mStbc = 0
Index  26, RAM Address  130 -  134 :   11ax datarate    2.6 Mbps @ rate 2, mStbc = 0
Index  27, RAM Address  135 -  139 :   11ax datarate    5.3 Mbps @ rate 2, mStbc = 0
Index  28, RAM Address  140 -  144 :   11ax datarate    7.9 Mbps @ rate 2, mStbc = 0
Index  29, RAM Address  145 -  149 :   11ax datarate   10.6 Mbps @ rate 2, mStbc = 0
Index  30, RAM Address  150 -  154 :   11ax datarate   11.2 Mbps @ rate 2, mStbc = 0
Index  31, RAM Address  155 -  159 :   11ax datarate   15.9 Mbps @ rate 2, mStbc = 0
Index  32, RAM Address  160 -  164 :   11ax datarate   21.2 Mbps @ rate 2, mStbc = 0
Index  33, RAM Address  165 -  169 :   11ax datarate   22.5 Mbps @ rate 2, mStbc = 0
Index  34, RAM Address  170 -  174 :   11ax datarate   25.8 Mbps @ rate 2, mStbc = 0
Index  35, RAM Address  175 -  179 :   11ax datarate   33.8 Mbps @ rate 2, mStbc = 0
Index  36, RAM Address  180 -  184 :   11ax datarate   45.0 Mbps @ rate 2, mStbc = 0
Index  37, RAM Address  185 -  189 :   11ax datarate   51.6 Mbps @ rate 2, mStbc = 0
Index  38, RAM Address  190 -  194 :   11ax datarate   77.4 Mbps @ rate 2, mStbc = 0
Index  39, RAM Address  195 -  199 :   11ax datarate  103.2 Mbps @ rate 2, mStbc = 0
Index  40, RAM Address  200 -  204 :   11ax datarate  129.0 Mbps @ rate 2, mStbc = 0
Index  41, RAM Address  205 -  209 :   11ax datarate    8.8 Mbps @ rate 3, mStbc = 0
Index  42, RAM Address  210 -  214 :   11ax datarate   11.8 Mbps @ rate 3, mStbc = 0
Index  43, RAM Address  215 -  219 :   11ax datarate   17.6 Mbps @ rate 3, mStbc = 0
Index  44, RAM Address  220 -  224 :   11ax datarate   23.5 Mbps @ rate 3, mStbc = 0
Index  45, RAM Address  225 -  229 :   11ax datarate   37.5 Mbps @ rate 3, mStbc = 0
Index  46, RAM Address  230 -  234 :   11ax datarate   50.0 Mbps @ rate 3, mStbc = 0
Index  47, RAM Address  235 -  239 :   11ax datarate   86.0 Mbps @ rate 3, mStbc = 0
Index  48, RAM Address  240 -  244 :   11ax datarate  114.7 Mbps @ rate 3, mStbc = 0
Index  49, RAM Address  245 -  249 :   11ax datarate  143.4 Mbps @ rate 3, mStbc = 0
------------------------------------------------------------------------------------
--------------------- Entries for 1x1 40 MHz 11n/ac/ax no STBC ---------------------
------------------------------------------------------------------------------------
Index  50, RAM Address  250 -  254 : 11n/ac datarate   30.0 Mbps @ rate 0, mStbc = 0
Index  51, RAM Address  255 -  259 : 11n/ac datarate   60.0 Mbps @ rate 0, mStbc = 0
Index  52, RAM Address  260 -  264 : 11n/ac datarate  120.0 Mbps @ rate 1, mStbc = 0
Index  53, RAM Address  265 -  269 : 11n/ac datarate   45.0 Mbps @ rate 2, mStbc = 0
Index  54, RAM Address  270 -  274 : 11n/ac datarate   90.0 Mbps @ rate 2, mStbc = 0
Index  55, RAM Address  275 -  279 : 11n/ac datarate  135.0 Mbps @ rate 2, mStbc = 0
Index  56, RAM Address  280 -  284 : 11n/ac datarate  180.0 Mbps @ rate 2, mStbc = 0
Index  57, RAM Address  285 -  289 : 11n/ac datarate  150.0 Mbps @ rate 3, mStbc = 0
Index  58, RAM Address  290 -  294 : 11n/ac datarate  200.0 Mbps @ rate 3, mStbc = 0
Index  59, RAM Address  295 -  299 :   11ax datarate   68.8 Mbps @ rate 0, mStbc = 0
Index  60, RAM Address  300 -  304 :   11ax datarate  137.6 Mbps @ rate 1, mStbc = 0
Index  61, RAM Address  305 -  309 :   11ax datarate  154.9 Mbps @ rate 2, mStbc = 0
Index  62, RAM Address  310 -  314 :   11ax datarate  206.5 Mbps @ rate 2, mStbc = 0
Index  63, RAM Address  315 -  319 :   11ax datarate  258.1 Mbps @ rate 2, mStbc = 0
Index  64, RAM Address  320 -  324 :   11ax datarate  172.1 Mbps @ rate 3, mStbc = 0
Index  65, RAM Address  325 -  329 :   11ax datarate  229.4 Mbps @ rate 3, mStbc = 0
Index  66, RAM Address  330 -  334 :   11ax datarate  286.8 Mbps @ rate 3, mStbc = 0
------------------------------------------------------------------------------------
------------------- Entries for 1x1 20/40 MHz 11n/ac/ax with STBC ------------------
------------------------------------------------------------------------------------
Index  67, RAM Address  335 -  339 : 11n/ac datarate    8.0 Mbps @ rate 0, mStbc = 1
Index  68, RAM Address  340 -  344 : 11n/ac datarate   15.0 Mbps @ rate 0, mStbc = 1
Index  69, RAM Address  345 -  349 : 11n/ac datarate   29.0 Mbps @ rate 0, mStbc = 1
Index  70, RAM Address  350 -  354 : 11n/ac datarate   58.0 Mbps @ rate 1, mStbc = 1
Index  71, RAM Address  355 -  359 : 11n/ac datarate   22.0 Mbps @ rate 2, mStbc = 1
Index  72, RAM Address  360 -  364 : 11n/ac datarate   44.0 Mbps @ rate 2, mStbc = 1
Index  73, RAM Address  365 -  369 : 11n/ac datarate   65.0 Mbps @ rate 2, mStbc = 1
Index  74, RAM Address  370 -  374 : 11n/ac datarate   87.0 Mbps @ rate 2, mStbc = 1
Index  75, RAM Address  375 -  379 : 11n/ac datarate   73.0 Mbps @ rate 3, mStbc = 1
Index  76, RAM Address  380 -  384 :   11ax datarate    0.4 Mbps @ rate 0, mStbc = 1
Index  77, RAM Address  385 -  389 :   11ax datarate    0.9 Mbps @ rate 0, mStbc = 1
Index  78, RAM Address  390 -  394 :   11ax datarate    1.8 Mbps @ rate 0, mStbc = 1
Index  79, RAM Address  395 -  399 :   11ax datarate    1.9 Mbps @ rate 0, mStbc = 1
Index  80, RAM Address  400 -  404 :   11ax datarate    3.5 Mbps @ rate 0, mStbc = 1
Index  81, RAM Address  405 -  409 :   11ax datarate    3.7 Mbps @ rate 0, mStbc = 1
Index  82, RAM Address  410 -  414 :   11ax datarate    4.3 Mbps @ rate 0, mStbc = 1
Index  83, RAM Address  415 -  419 :   11ax datarate    7.1 Mbps @ rate 0, mStbc = 1
Index  84, RAM Address  420 -  424 :   11ax datarate    7.5 Mbps @ rate 0, mStbc = 1
Index  85, RAM Address  425 -  429 :   11ax datarate    8.6 Mbps @ rate 0, mStbc = 1
Index  86, RAM Address  430 -  434 :   11ax datarate   15.0 Mbps @ rate 0, mStbc = 1
Index  87, RAM Address  435 -  439 :   11ax datarate   17.2 Mbps @ rate 0, mStbc = 1
Index  88, RAM Address  440 -  444 :   11ax datarate   34.4 Mbps @ rate 0, mStbc = 1
Index  89, RAM Address  445 -  449 :   11ax datarate    7.1 Mbps @ rate 1, mStbc = 1
Index  90, RAM Address  450 -  454 :   11ax datarate   14.1 Mbps @ rate 1, mStbc = 1
Index  91, RAM Address  455 -  459 :   11ax datarate   30.0 Mbps @ rate 1, mStbc = 1
Index  92, RAM Address  460 -  464 :   11ax datarate   68.8 Mbps @ rate 1, mStbc = 1
Index  93, RAM Address  465 -  469 :   11ax datarate    2.6 Mbps @ rate 2, mStbc = 1
Index  94, RAM Address  470 -  474 :   11ax datarate    5.3 Mbps @ rate 2, mStbc = 1
Index  95, RAM Address  475 -  479 :   11ax datarate    7.9 Mbps @ rate 2, mStbc = 1
Index  96, RAM Address  480 -  484 :   11ax datarate   10.6 Mbps @ rate 2, mStbc = 1
Index  97, RAM Address  485 -  489 :   11ax datarate   11.2 Mbps @ rate 2, mStbc = 1
Index  98, RAM Address  490 -  494 :   11ax datarate   15.9 Mbps @ rate 2, mStbc = 1
Index  99, RAM Address  495 -  499 :   11ax datarate   21.2 Mbps @ rate 2, mStbc = 1
Index 100, RAM Address  500 -  504 :   11ax datarate   22.5 Mbps @ rate 2, mStbc = 1
Index 101, RAM Address  505 -  509 :   11ax datarate   25.8 Mbps @ rate 2, mStbc = 1
Index 102, RAM Address  510 -  514 :   11ax datarate   33.8 Mbps @ rate 2, mStbc = 1
Index 103, RAM Address  515 -  519 :   11ax datarate   45.0 Mbps @ rate 2, mStbc = 1
Index 104, RAM Address  520 -  524 :   11ax datarate   51.6 Mbps @ rate 2, mStbc = 1
Index 105, RAM Address  525 -  529 :   11ax datarate   77.4 Mbps @ rate 2, mStbc = 1
Index 106, RAM Address  530 -  534 :   11ax datarate  103.2 Mbps @ rate 2, mStbc = 1
Index 107, RAM Address  535 -  539 :   11ax datarate  129.0 Mbps @ rate 2, mStbc = 1
Index 108, RAM Address  540 -  544 :   11ax datarate    8.8 Mbps @ rate 3, mStbc = 1
Index 109, RAM Address  545 -  549 :   11ax datarate   11.8 Mbps @ rate 3, mStbc = 1
Index 110, RAM Address  550 -  554 :   11ax datarate   17.6 Mbps @ rate 3, mStbc = 1
Index 111, RAM Address  555 -  559 :   11ax datarate   23.5 Mbps @ rate 3, mStbc = 1
Index 112, RAM Address  560 -  564 :   11ax datarate   37.5 Mbps @ rate 3, mStbc = 1
Index 113, RAM Address  565 -  569 :   11ax datarate   50.0 Mbps @ rate 3, mStbc = 1
Index 114, RAM Address  570 -  574 :   11ax datarate   86.0 Mbps @ rate 3, mStbc = 1
Index 115, RAM Address  575 -  579 :   11ax datarate  114.7 Mbps @ rate 3, mStbc = 1
Index 116, RAM Address  580 -  584 :   11ax datarate  143.4 Mbps @ rate 3, mStbc = 1
Index 117, RAM Address  585 -  589 : 11n/ac datarate   30.0 Mbps @ rate 0, mStbc = 1
Index 118, RAM Address  590 -  594 : 11n/ac datarate   60.0 Mbps @ rate 0, mStbc = 1
Index 119, RAM Address  595 -  599 : 11n/ac datarate  120.0 Mbps @ rate 1, mStbc = 1
Index 120, RAM Address  600 -  604 : 11n/ac datarate   45.0 Mbps @ rate 2, mStbc = 1
Index 121, RAM Address  605 -  609 : 11n/ac datarate   90.0 Mbps @ rate 2, mStbc = 1
Index 122, RAM Address  610 -  614 : 11n/ac datarate  135.0 Mbps @ rate 2, mStbc = 1
Index 123, RAM Address  615 -  619 : 11n/ac datarate  180.0 Mbps @ rate 2, mStbc = 1
Index 124, RAM Address  620 -  624 : 11n/ac datarate  150.0 Mbps @ rate 3, mStbc = 1
Index 125, RAM Address  625 -  629 : 11n/ac datarate  200.0 Mbps @ rate 3, mStbc = 1
Index 126, RAM Address  630 -  634 :   11ax datarate   68.8 Mbps @ rate 0, mStbc = 1
Index 127, RAM Address  635 -  639 :   11ax datarate  137.6 Mbps @ rate 1, mStbc = 1
Index 128, RAM Address  640 -  644 :   11ax datarate  154.9 Mbps @ rate 2, mStbc = 1
Index 129, RAM Address  645 -  649 :   11ax datarate  206.5 Mbps @ rate 2, mStbc = 1
Index 130, RAM Address  650 -  654 :   11ax datarate  258.1 Mbps @ rate 2, mStbc = 1
Index 131, RAM Address  655 -  659 :   11ax datarate  172.1 Mbps @ rate 3, mStbc = 1
Index 132, RAM Address  660 -  664 :   11ax datarate  229.4 Mbps @ rate 3, mStbc = 1
Index 133, RAM Address  665 -  669 :   11ax datarate  286.8 Mbps @ rate 3, mStbc = 1
------------------------------------------------------------------------------------
-------------- Entries for 1x1 80 MHz 11n/ac/ax with and without STBC --------------
------------------------------------------------------------------------------------
Index 134, RAM Address  670 -  674 : 11n/ac datarate   33.0 Mbps @ rate 0, mStbc = 0
Index 135, RAM Address  675 -  679 : 11n/ac datarate   65.0 Mbps @ rate 0, mStbc = 0
Index 136, RAM Address  680 -  684 : 11n/ac datarate  130.0 Mbps @ rate 0, mStbc = 0
Index 137, RAM Address  685 -  689 : 11n/ac datarate  260.0 Mbps @ rate 1, mStbc = 0
Index 138, RAM Address  690 -  694 : 11n/ac datarate   98.0 Mbps @ rate 2, mStbc = 0
Index 139, RAM Address  695 -  699 : 11n/ac datarate  195.0 Mbps @ rate 2, mStbc = 0
Index 140, RAM Address  700 -  704 : 11n/ac datarate  293.0 Mbps @ rate 2, mStbc = 0
Index 141, RAM Address  705 -  709 : 11n/ac datarate  390.0 Mbps @ rate 2, mStbc = 0
Index 142, RAM Address  710 -  714 : 11n/ac datarate  325.0 Mbps @ rate 3, mStbc = 0
Index 143, RAM Address  715 -  719 : 11n/ac datarate  434.0 Mbps @ rate 3, mStbc = 0
Index 144, RAM Address  720 -  724 :   11ax datarate   18.0 Mbps @ rate 0, mStbc = 0
Index 145, RAM Address  725 -  729 :   11ax datarate   36.0 Mbps @ rate 0, mStbc = 0
Index 146, RAM Address  730 -  734 :   11ax datarate   72.1 Mbps @ rate 0, mStbc = 0
Index 147, RAM Address  735 -  739 :   11ax datarate  144.1 Mbps @ rate 0, mStbc = 0
Index 148, RAM Address  740 -  744 :   11ax datarate  288.2 Mbps @ rate 1, mStbc = 0
Index 149, RAM Address  745 -  749 :   11ax datarate  108.1 Mbps @ rate 2, mStbc = 0
Index 150, RAM Address  750 -  754 :   11ax datarate  216.2 Mbps @ rate 2, mStbc = 0
Index 151, RAM Address  755 -  759 :   11ax datarate  324.3 Mbps @ rate 2, mStbc = 0
Index 152, RAM Address  760 -  764 :   11ax datarate  432.4 Mbps @ rate 2, mStbc = 0
Index 153, RAM Address  765 -  769 :   11ax datarate  540.4 Mbps @ rate 2, mStbc = 0
Index 154, RAM Address  770 -  774 :   11ax datarate  360.3 Mbps @ rate 3, mStbc = 0
Index 155, RAM Address  775 -  779 :   11ax datarate  480.4 Mbps @ rate 3, mStbc = 0
Index 156, RAM Address  780 -  784 :   11ax datarate  600.5 Mbps @ rate 3, mStbc = 0
Index 157, RAM Address  785 -  789 : 11n/ac datarate   33.0 Mbps @ rate 0, mStbc = 1
Index 158, RAM Address  790 -  794 : 11n/ac datarate   65.0 Mbps @ rate 0, mStbc = 1
Index 159, RAM Address  795 -  799 : 11n/ac datarate  130.0 Mbps @ rate 0, mStbc = 1
Index 160, RAM Address  800 -  804 : 11n/ac datarate  260.0 Mbps @ rate 1, mStbc = 1
Index 161, RAM Address  805 -  809 : 11n/ac datarate   98.0 Mbps @ rate 2, mStbc = 1
Index 162, RAM Address  810 -  814 : 11n/ac datarate  195.0 Mbps @ rate 2, mStbc = 1
Index 163, RAM Address  815 -  819 : 11n/ac datarate  293.0 Mbps @ rate 2, mStbc = 1
Index 164, RAM Address  820 -  824 : 11n/ac datarate  390.0 Mbps @ rate 2, mStbc = 1
Index 165, RAM Address  825 -  829 : 11n/ac datarate  325.0 Mbps @ rate 3, mStbc = 1
Index 166, RAM Address  830 -  834 : 11n/ac datarate  434.0 Mbps @ rate 3, mStbc = 1
Index 167, RAM Address  835 -  839 :   11ax datarate   18.0 Mbps @ rate 0, mStbc = 1
Index 168, RAM Address  840 -  844 :   11ax datarate   36.0 Mbps @ rate 0, mStbc = 1
Index 169, RAM Address  845 -  849 :   11ax datarate   72.1 Mbps @ rate 0, mStbc = 1
Index 170, RAM Address  850 -  854 :   11ax datarate  144.1 Mbps @ rate 0, mStbc = 1
Index 171, RAM Address  855 -  859 :   11ax datarate  288.2 Mbps @ rate 1, mStbc = 1
Index 172, RAM Address  860 -  864 :   11ax datarate  108.1 Mbps @ rate 2, mStbc = 1
Index 173, RAM Address  865 -  869 :   11ax datarate  216.2 Mbps @ rate 2, mStbc = 1
Index 174, RAM Address  870 -  874 :   11ax datarate  324.3 Mbps @ rate 2, mStbc = 1
Index 175, RAM Address  875 -  879 :   11ax datarate  432.4 Mbps @ rate 2, mStbc = 1
Index 176, RAM Address  880 -  884 :   11ax datarate  540.4 Mbps @ rate 2, mStbc = 1
Index 177, RAM Address  885 -  889 :   11ax datarate  360.3 Mbps @ rate 3, mStbc = 1
Index 178, RAM Address  890 -  894 :   11ax datarate  480.4 Mbps @ rate 3, mStbc = 1
Index 179, RAM Address  895 -  899 :   11ax datarate  600.5 Mbps @ rate 3, mStbc = 1
------------------------------------------------------------------------------------
------------------- Entries for 2x2 20/40/80 MHz 11n/ac/ax no STBC ------------------
------------------------------------------------------------------------------------
Index 180, RAM Address  900 -  904 : 11n/ac datarate   58.0 Mbps @ rate 0, mStbc = 0
Index 181, RAM Address  905 -  909 : 11n/ac datarate  120.0 Mbps @ rate 0, mStbc = 0
Index 182, RAM Address  910 -  914 : 11n/ac datarate  260.0 Mbps @ rate 0, mStbc = 0
Index 183, RAM Address  915 -  919 : 11n/ac datarate  116.0 Mbps @ rate 1, mStbc = 0
Index 184, RAM Address  920 -  924 : 11n/ac datarate  240.0 Mbps @ rate 1, mStbc = 0
Index 185, RAM Address  925 -  929 : 11n/ac datarate  520.0 Mbps @ rate 1, mStbc = 0
Index 186, RAM Address  930 -  934 : 11n/ac datarate  130.0 Mbps @ rate 2, mStbc = 0
Index 187, RAM Address  935 -  939 : 11n/ac datarate  174.0 Mbps @ rate 2, mStbc = 0
Index 188, RAM Address  940 -  944 : 11n/ac datarate  270.0 Mbps @ rate 2, mStbc = 0
Index 189, RAM Address  945 -  949 : 11n/ac datarate  360.0 Mbps @ rate 2, mStbc = 0
Index 190, RAM Address  950 -  954 : 11n/ac datarate  585.0 Mbps @ rate 2, mStbc = 0
Index 191, RAM Address  955 -  959 : 11n/ac datarate  780.0 Mbps @ rate 2, mStbc = 0
Index 192, RAM Address  960 -  964 : 11n/ac datarate  145.0 Mbps @ rate 3, mStbc = 0
Index 193, RAM Address  965 -  969 : 11n/ac datarate  300.0 Mbps @ rate 3, mStbc = 0
Index 194, RAM Address  970 -  974 : 11n/ac datarate  400.0 Mbps @ rate 3, mStbc = 0
Index 195, RAM Address  975 -  979 : 11n/ac datarate  650.0 Mbps @ rate 3, mStbc = 0
Index 196, RAM Address  980 -  984 : 11n/ac datarate  867.0 Mbps @ rate 3, mStbc = 0
Index 197, RAM Address  985 -  989 :   11ax datarate   14.1 Mbps @ rate 0, mStbc = 0
Index 198, RAM Address  990 -  994 :   11ax datarate   30.0 Mbps @ rate 0, mStbc = 0
Index 199, RAM Address  995 -  999 :   11ax datarate  137.6 Mbps @ rate 0, mStbc = 0
Index 200, RAM Address 1000 - 1004 :   11ax datarate  288.2 Mbps @ rate 0, mStbc = 0
Index 201, RAM Address 1005 - 1009 :   11ax datarate   28.2 Mbps @ rate 1, mStbc = 0
Index 202, RAM Address 1010 - 1014 :   11ax datarate   60.0 Mbps @ rate 1, mStbc = 0
Index 203, RAM Address 1015 - 1019 :   11ax datarate  275.3 Mbps @ rate 1, mStbc = 0
Index 204, RAM Address 1020 - 1024 :   11ax datarate  576.5 Mbps @ rate 1, mStbc = 0
Index 205, RAM Address 1025 - 1029 :   11ax datarate   31.8 Mbps @ rate 2, mStbc = 0
Index 206, RAM Address 1030 - 1034 :   11ax datarate   42.4 Mbps @ rate 2, mStbc = 0
Index 207, RAM Address 1035 - 1039 :   11ax datarate   67.5 Mbps @ rate 2, mStbc = 0
Index 208, RAM Address 1040 - 1044 :   11ax datarate   90.0 Mbps @ rate 2, mStbc = 0
Index 209, RAM Address 1045 - 1049 :   11ax datarate  309.7 Mbps @ rate 2, mStbc = 0
Index 210, RAM Address 1050 - 1054 :   11ax datarate  412.9 Mbps @ rate 2, mStbc = 0
Index 211, RAM Address 1055 - 1059 :   11ax datarate  516.2 Mbps @ rate 2, mStbc = 0
Index 212, RAM Address 1060 - 1064 :   11ax datarate  648.5 Mbps @ rate 2, mStbc = 0
Index 213, RAM Address 1065 - 1069 :   11ax datarate  864.7 Mbps @ rate 2, mStbc = 0
Index 214, RAM Address 1070 - 1074 :   11ax datarate 1080.9 Mbps @ rate 2, mStbc = 0
Index 215, RAM Address 1075 - 1079 :   11ax datarate   35.3 Mbps @ rate 3, mStbc = 0
Index 216, RAM Address 1080 - 1084 :   11ax datarate   47.1 Mbps @ rate 3, mStbc = 0
Index 217, RAM Address 1085 - 1089 :   11ax datarate   75.0 Mbps @ rate 3, mStbc = 0
Index 218, RAM Address 1090 - 1094 :   11ax datarate  100.0 Mbps @ rate 3, mStbc = 0
Index 219, RAM Address 1095 - 1099 :   11ax datarate  344.1 Mbps @ rate 3, mStbc = 0
Index 220, RAM Address 1100 - 1104 :   11ax datarate  458.8 Mbps @ rate 3, mStbc = 0
Index 221, RAM Address 1105 - 1109 :   11ax datarate  573.5 Mbps @ rate 3, mStbc = 0
Index 222, RAM Address 1110 - 1114 :   11ax datarate  720.6 Mbps @ rate 3, mStbc = 0
Index 223, RAM Address 1115 - 1119 :   11ax datarate  960.8 Mbps @ rate 3, mStbc = 0
Index 224, RAM Address 1120 - 1124 :   11ax datarate 1201.0 Mbps @ rate 3, mStbc = 0
