# mm_set_ps_options_req Struct Reference
[MM_TASK]

Structure containing the parameters of the MM_SET_PS_OPTIONS_REQ message. More...

`#include <mm_task.h>`

## Data Fields
uint8_t | vif_index
| VIF Index.
uint16_t | listen_interval
| Listen interval (0 if wake up shall be based on DTIM period).
bool | dont_listen_bc_mc
| Flag indicating if we shall listen the BC/MC traffic or not.

## Detailed Description

Structure containing the parameters of the MM_SET_PS_OPTIONS_REQ message.

Definition at line 864 of file mm_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/mm/mm_task.h