# me_rc_stats_cfm Struct Reference
[TASK_ME]

Structure containing the parameters of the ME_RC_STATS_CFM message. More...

`#include <me_task.h>`

Collaboration diagram for me_rc_stats_cfm:
[legend]

## Data Fields
uint8_t | sta_idx
| Index of the station for which the RC statistics are provided.
uint16_t | no_samples
| Number of samples used in the RC algorithm.
uint16_t | ampdu_len
| Number of MPDUs transmitted (per sampling interval).
uint16_t | ampdu_packets
| Number of AMPDUs transmitted (per sampling interval).
uint32_t | avg_ampdu_len
| Average number of MPDUs in each AMPDU frame (EWMA).
uint8_t | sw_retry_step
| Current step 0 of the retry chain.
uint8_t | sample_wait
| Trial transmission period.
uint16_t | retry_step_idx [RATE_CONTROL_STEPS]
| Retry chain steps.
struct rc_rate_stats | rate_stats [RC_MAX_N_SAMPLE+1]
| RC statistics - Max number of RC samples, plus one for the HE TB statistics.
uint32_t | tp [RC_MAX_N_SAMPLE+1]
| Throughput - Max number of RC samples, plus one for the HE TB statistics.

## Detailed Description

Structure containing the parameters of the ME_RC_STATS_CFM message.

Definition at line 272 of file me_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/me/me_task.h