# mic_calc Struct Reference
[MIC_CALC]

========================== Context Definition =========================== This structure contains the attributes that defines the current state of the MIC key Calculator More...

`#include <me_mic.h>`

## Data Fields
uint32_t | mic_key_least
| Holds the 1st 4 bytes of the intermediate MIC key during the calculation process (little-end).
uint32_t | mic_key_most
| Holds the last 4 bytes of the intermediate MIC key during the calculation process (little-end).
uint32_t | last_m_i
| Contain the latest incomplete M(i) block.
uint8_t | last_m_i_len
| Length of M(i) that has already been received.

## Detailed Description

========================== Context Definition =========================== This structure contains the attributes that defines the current state of the MIC key Calculator

Definition at line 42 of file me_mic.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/me/me_mic.h