# txl_cntrl_env_tag Struct Reference
[TX_CNTRL]

Context of the Tx Control block. More...

`#include <txl_cntrl.h>`

Collaboration diagram for txl_cntrl_env_tag:
[legend]

## Data Fields
struct txl_list | txlist [NX_TXQ_CNT]
| Transmission list per AC.
uint32_t | pck_cnt
| Number of packets currently in the TX path.
uint16_t | mumimo_ppdu_cnt
| MU-MIMO PPDUs currently chained to HW.
uint16_t | seqnbr
| Non-QoS sequence number.
bool | reset
| Indicate if we are resetting the TX path.

## Detailed Description

Context of the Tx Control block.

Definition at line 257 of file txl_cntrl.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/tx/txl/txl_cntrl.h