# mm_channel_survey_ind Struct Reference
[MM_TASK]

Structure containing the parameters of the MM_CHANNEL_SURVEY_IND message. More...

`#include <mm_task.h>`

## Data Fields
uint16_t | freq
| Frequency of the channel.
int8_t | noise_dbm
| Noise in dbm.
uint32_t | chan_time_ms
| Amount of time spent on the channel (in ms).
uint32_t | chan_time_busy_ms
| Amount of time the primary channel was sensed busy.

## Detailed Description

Structure containing the parameters of the MM_CHANNEL_SURVEY_IND message.

Definition at line 884 of file mm_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/mm/mm_task.h