# mm_key_add_req Struct Reference
[MM_TASK]

Structure containing the parameters of the MM_KEY_ADD_REQ message. More...

`#include <mm_task.h>`

Collaboration diagram for mm_key_add_req:
[legend]

## Data Fields
uint8_t | key_idx
| Key index (valid only for default keys).
uint8_t | sta_idx
| STA index (valid only for pairwise keys or mesh group keys).
struct mac_sec_key | key
| Key material.
uint8_t | cipher_suite
| Cipher suite (WEP64, WEP128, TKIP, CCMP).
uint8_t | inst_nbr
| Index of the interface for which the key is set (valid only for default keys or mesh group keys).
uint8_t | spp
| A-MSDU SPP parameter.
bool | pairwise
| Indicate if provided key is a pairwise key or not.

## Detailed Description

Structure containing the parameters of the MM_KEY_ADD_REQ message.

Definition at line 578 of file mm_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/mm/mm_task.h