# mm_set_edca_req Struct Reference
[MM_TASK]

Structure containing the parameters of the MM_SET_EDCA_REQ message. More...

`#include <mm_task.h>`

## Data Fields
uint32_t | ac_param
| EDCA parameters of the queue (as expected by edcaACxReg HW register).
bool | uapsd
| Flag indicating if UAPSD can be used on this queue.
uint8_t | hw_queue
| HW queue for which the parameters are configured.
uint8_t | inst_nbr
| Index of the interface for which the parameters are configured.

## Detailed Description

Structure containing the parameters of the MM_SET_EDCA_REQ message.

Definition at line 408 of file mm_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/mm/mm_task.h