# mac_chan_op Struct Reference
[MAC]

Operating Channel. More...

`#include <mac_types.h>`

## Data Fields
uint8_t | band
| Band (mac_chan_band).
uint8_t | type
| Channel type (mac_chan_bandwidth).
uint16_t | prim20_freq
| Frequency for Primary 20MHz channel (in MHz).
uint16_t | center1_freq
| Frequency center of the contiguous channel or center of Primary 80+80 (in MHz).
uint16_t | center2_freq
| Frequency center of the non-contiguous secondary 80+80 (in MHz).
int8_t | tx_power
| Max transmit power allowed on this channel (dBm).
uint8_t | flags
| Additional information (mac_chan_flags).

## Detailed Description

Operating Channel.

Definition at line 138 of file mac_types.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/modules/mac/src/mac_types.h