# /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/hal/hal_desc.c File Reference

File containing the definition of HW descriptors. More...

`#include "hal_desc.h"`
`#include "tx_swdesc.h"`
`#include "hal_machw_mib.h"`
`#include "compiler.h"`

Go to the source code of this file.

## Variables
struct tx_hw_desc | tx_hw_desc0 [RW_USER_MAX *NX_TXDESC_CNT0]
| Array of HW descriptors for BK queue.
struct tx_hw_desc | tx_hw_desc1 [RW_USER_MAX *NX_TXDESC_CNT1]
| Array of HW descriptors for BE queue.
struct tx_hw_desc | tx_hw_desc2 [RW_USER_MAX *NX_TXDESC_CNT2]
| Array of HW descriptors for VI queue.
struct tx_hw_desc | tx_hw_desc3 [RW_USER_MAX *NX_TXDESC_CNT3]
| Array of HW descriptors for VO queue.
struct tx_hw_desc | tx_hw_desc4 [NX_TXDESC_CNT4]
| Array of HW descriptors for BCN queue.
struct dma_desc | bcn_dwnld_desc
| IPC DMA control structure for beacon download.

## Detailed Description

File containing the definition of HW descriptors.

File containing the definition of the structure and API function used to initialize the pool.

Copyright (C) RivieraWaves 2011-2019

Definition in file hal_desc.c.