# sta_mgmt_ba_info Struct Reference
[STA_MGMT]

Information about RX and TX Block Ack for one TID. More...

`#include <sta_mgmt.h>`

## Data Fields
uint32_t | last_ba_add_time
| Last time a ADD BA request has been attempted.
uint8_t | bam_idx_rx
| BAM task instance (RX Side).
uint8_t | bam_idx_tx
| BAM task instance (TX Side).
int8_t | credit_oft
| Offset to apply to the credit count of this STA/TID pair.
uint8_t | tx_pkt_cnt
| Number of frames currently in the TX path for this STA/TID pair.

## Detailed Description

Information about RX and TX Block Ack for one TID.

Definition at line 272 of file sta_mgmt.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/sta/sta_mgmt.h