# /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/me/me_task.c File Reference

The UMAC's ME (MAC Layer Management Entity) module implementation. More...

`#include "me_task.h"`
`#include "me.h"`
`#include "mm.h"`
`#include "me_utils.h"`
`#include "scan_task.h"`
`#include "dbg.h"`
`#include "rxu_task.h"`
`#include "sta_mgmt.h"`
`#include "vif_mgmt.h"`
`#include "ps.h"`
`#include "co_endian.h"`

Go to the source code of this file.

## Functions
static int | me_config_req_handler (ke_msg_id_t const msgid, struct me_config_req const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| ME module message handler.
static int | me_chan_config_req_handler (ke_msg_id_t const msgid, struct me_chan_config_req const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| ME module message handler.
static int | me_set_control_port_req_handler (ke_msg_id_t const msgid, struct me_set_control_port_req const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| ME module message handler.
static int | me_sta_add_req_handler (ke_msg_id_t const msgid, struct me_sta_add_req const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| ME module message handler.
static int | me_sta_del_req_handler (ke_msg_id_t const msgid, struct me_sta_del_req const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| ME module message handler.
static int | me_traffic_ind_req_handler (ke_msg_id_t const msgid, struct me_traffic_ind_req const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| ME module message handler.
static int | me_set_active_req_handler (ke_msg_id_t const msgid, struct me_set_active_req const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| ME module message handler.
static int | mm_set_idle_cfm_handler (ke_msg_id_t const msgid, void const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| ME module message handler.
static int | me_set_ps_disable_req_handler (ke_msg_id_t const msgid, struct me_set_ps_disable_req const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| ME module message handler.
static int | me_set_ps_mode_req_handler (ke_msg_id_t const msgid, struct me_set_ps_mode_req const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| ME module message handler.
static int | mm_set_ps_mode_cfm_handler (ke_msg_id_t const msgid, void const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| ME module message handler.
static int | me_rc_stats_req_handler (ke_msg_id_t const msgid, struct me_rc_stats_req const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| RC module message handler.
static int | me_rc_set_rate_req_handler (ke_msg_id_t const msgid, struct me_rc_set_rate_req const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| RC module message handler.
static int | me_config_monitor_req_handler (ke_msg_id_t const msgid, struct me_config_monitor_req const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| ME module message handler.
## Variables
struct ke_msg_handler | me_default_state []
| DEFAULT handler definition.
struct ke_state_handler | me_default_handler = KE_STATE_HANDLER(me_default_state)
| Specifies the message handlers that are common to all states.
ke_state_t | me_state [ME_IDX_MAX]
| Defines the place holder for the states of all the task instances.

## Detailed Description

The UMAC's ME (MAC Layer Management Entity) module implementation.

Copyright (C) RivieraWaves 2011-2019

Definition in file me_task.c.