# sm_connect_cfm Struct Reference
[TASK_SM]

Structure containing the parameters of the SM_CONNECT_CFM message. More...

`#include <sm_task.h>`

## Data Fields
uint8_t | status
| Status.

## Detailed Description

Structure containing the parameters of the SM_CONNECT_CFM message.

Definition at line 114 of file sm_task.h.

## Field Documentation

uint8_t sm_connect_cfm::status

Status.

If 0, it means that the connection procedure will be performed and that a subsequent SM_CONNECT_IND message will be forwarded once the procedure is completed.

Definition at line 119 of file sm_task.h.

Referenced by sm_connect_req_handler().

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/sm/sm_task.h