# scan_probe_req_ie_tag Struct Reference
[SCAN]

Definition of a ProbeReq IE buffer. More...

`#include <scan.h>`

Collaboration diagram for scan_probe_req_ie_tag:
[legend]

## Data Fields
struct dma_desc | dma_desc
| DMA descriptor to download the IEs from host memory.
struct tx_pbd | pbd
| TX payload buffer descriptor.
uint32_t | buf [SCAN_MAX_IE_LEN/4]
| Buffer space for IEs.

## Detailed Description

Definition of a ProbeReq IE buffer.

Definition at line 61 of file scan.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/scan/scan.h