C8051F342

## USB005-specific pins

P00	SDA
P01	SCL
P02	status LED ?

### Unused in I2C mode

P04	FPGA ??
P05	FPGA ??
P06	FPGA SDA
P07	FPGA SCL

## USB/power pins

see i.e. http://akb77.com/g/silabs/jump-to-silabs-step-1/TSDAS.png

REGIN -	USB VBUS
VBUS - USB VBUS
D+	- USB D+
D-	- USB D-
GND	GND

