---
UID: NS:bluetoothapis._BLUETOOTH_ADDRESS
title: BLUETOOTH_ADDRESS_STRUCT (bluetoothapis.h)
description: The BLUETOOTH_ADDRESS structure provides the address of a Bluetooth device.
old-location: bluetooth\bluetooth_address.htm
tech.root: bluetooth
ms.assetid: 2262a91b-c8b0-415a-9c23-7504998cc2a4
ms.date: 12/05/2018
ms.keywords: BLUETOOTH_ADDRESS, BLUETOOTH_ADDRESS structure [Bluetooth], BLUETOOTH_ADDRESS_STRUCT, _BLUETOOTH_ADDRESS, _bth_bluetooth_address, bluetooth.bluetooth_address, bluetoothapis/BLUETOOTH_ADDRESS
f1_keywords:
- bluetoothapis/BLUETOOTH_ADDRESS
dev_langs:
- c++
req.header: bluetoothapis.h
req.include-header: Bthsdpdef.h, BluetoothAPIs.h
req.target-type: Windows
req.target-min-winverclnt: Windows Vista, Windows XP with SP2 [desktop apps only]
req.target-min-winversvr: None supported
req.kmdf-ver: 
req.umdf-ver: 
req.ddi-compliance: 
req.unicode-ansi: 
req.idl: 
req.max-support: 
req.namespace: 
req.assembly: 
req.type-library: 
req.lib: 
req.dll: 
req.irql: 
topic_type:
- APIRef
- kbSyntax
api_type:
- HeaderDef
api_location:
- BluetoothAPIs.h
api_name:
- BLUETOOTH_ADDRESS
targetos: Windows
req.typenames: BLUETOOTH_ADDRESS_STRUCT
req.redist: 
ms.custom: 19H1
---

# BLUETOOTH_ADDRESS_STRUCT structure


## -description


The 
<b>BLUETOOTH_ADDRESS</b> structure provides the address of a Bluetooth device.


## -struct-fields




### -field ullLong

Address of a Bluetooth device.


### -field rgBytes

Address of a Bluetooth device, expressed as an array of bytes.

